,Wattage Comments##OTHER##,Wattage##ELECTRICAL_WATTAGE##WATTS,WEIGHT##MASS##POUNDS_MASS,WATTAGE##ELECTRICAL_WATTAGE##WATTS,Voltage Loss##OTHER##,VOLTAGE RANGE V##OTHER##,VOLTAGE##ELECTRICAL_POTENTIAL##VOLTS,URL##OTHER##,Total Light Loss Factor##OTHER##,Tilt Angle##ANGLE##DECIMAL DEGREES,Temperature Loss##OTHER##,Temperature Color##OTHER##,TECHNICAL SHEET##OTHER##,Surface Depreciation Loss##OTHER##,Photometric Web File##OTHER##,PRODUCT SHEET##OTHER##,PRODUCT CODE##OTHER##,None##OTHER##,NOISE ABSORPTION COEFFICIENT (NRC)##OTHER##,Model##OTHER##,Manufacturer##OTHER##,MATERIAL DESCRIPTION##OTHER##,Luminous Intensity##ELECTRICAL_LUMINOUS_INTENSITY##CANDELAS,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Luminaire Dirt Depreciation##OTHER##,Light Loss Input Method##OTHER##,Light Loss Factor##OTHER##,Lamp Tilt Loss##OTHER##,Lamp Lumen Depreciation##OTHER##,Lamp##OTHER##,LIGHTING SPECIFICATION##OTHER##,Initial Light Intensity Input Method##OTHER##,Initial Intensity##OTHER##,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Initial Color##OTHER##,Illuminance##ELECTRICAL_ILLUMINANCE##LUX,HEIGHT##LENGTH##INCHES,FREQUENCY RANGE Hz##OTHER##,Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT,Dimming Lamp Color Temperature Shift##OTHER##,Description##OTHER##,Default Elevation##LENGTH##INCHES,DIAMETER##LENGTH##INCHES,Color Filter##OTHER##,CORD LENGTH CONTROL##LENGTH##INCHES,CORD LENGTH##LENGTH##INCHES,COLOR RENDERING INDEX##OTHER##,COEFFICIENT OF WEIGHTENED ACOUSTIC ABSORPTION (αw)##OTHER##,Ballast Loss##OTHER##,BIM USER MANUAL##OTHER##,BIM BADGE##OTHER##,BIM AUTHOR##OTHER##,At a distance##LENGTH##INCHES,Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,ASSEMBLY SHEET##OTHER##,ACCESSORY CODE##OTHER##,ACCESSORIES##OTHER##,ABSORPTION CLASSES##OTHER##
D71CL+D71/6DL_WHITE,,52.849740932642,16.800000000000,65.000000000000,1,120 V,120.000000000000,www.luceplanusa.com,1,-90.000000000000,1,0,https://www.luceplanusa.com/products/petale-suspension,1,Pétale_D716DL_42W LED DLM.IES,https://www.archiproducts.com/en/products/luceplan/led-fabric-pendant-lamp-petale_349494,1D710C0L0002,䕉乓㩁䵌㘭ⴳ〲㈰਍呛卅嵔㐠㠷㌷㘷㌳⸶റ嬊䅍啎䅆嵃倠䥈䥌卐䰠䝉呈义⁇呉䱁൙嬊啌䍍呁⁝䕐䅔䕌䐠ㄷ䱃਍䱛䵕义䥁䕒⁝䕐䅔䕌䐠ㄷ䱃਍呛卅䱔䉁⁝䡐䱉偉⁓䥌䡇䥔䝎䤠䅔奌਍䥛卓䕕䅄䕔⁝㜱䴠牡㈠㄰ശ嬊䱆十䅈䕒嵁〠〮㐷ㄲശ嬊䅌偍䅃嵔䰠䑅਍䱛䵁嵐䰠䑅ⴠ㐠⸴〰圠਍佛䡔剅⁝扁潳畬整倠潨潴敭牴൹吊䱉㵔低䕎਍‱ㄭㄠ〮㜠″‱‱′〭㌮〵ⴠ⸰㔳‰⸰㔱രㄊ〮‰⸱〰㐠⸴〰਍⸰〰㈠㔮‰⸵〰㜠㔮‰〱〮‰㈱㔮‰㔱〮‰㜱㔮‰〲〮‰㈲㔮‰਍㔲〮‰㜲㔮‰〳〮‰㈳㔮‰㔳〮‰㜳㔮‰〴〮‰㈴㔮‰㔴〮‰਍㜴㔮‰〵〮‰㈵㔮‰㔵〮‰㜵㔮‰〶〮‰㈶㔮‰㔶〮‰㜶㔮‰਍〷〮‰㈷㔮‰㔷〮‰㜷㔮‰〸〮‰㈸㔮‰㔸〮‰㜸㔮‰〹〮‰਍㈹㔮‰㔹〮‰㜹㔮‰〱⸰〰ㄠ㈰㔮‰〱⸵〰ㄠ㜰㔮‰ㄱ⸰〰ഠㄊ㈱㔮‰ㄱ⸵〰ㄠ㜱㔮‰㈱⸰〰ㄠ㈲㔮‰㈱⸵〰ㄠ㜲㔮‰㌱⸰〰ഠㄊ㈳㔮‰㌱⸵〰ㄠ㜳㔮‰㐱⸰〰ㄠ㈴㔮‰㐱⸵〰ㄠ㜴㔮‰㔱⸰〰ഠㄊ㈵㔮‰㔱⸵〰ㄠ㜵㔮‰㘱⸰〰ㄠ㈶㔮‰㘱⸵〰ㄠ㜶㔮‰㜱⸰〰ഠㄊ㈷㔮‰㜱⸵〰ㄠ㜷㔮‰㠱⸰〰ഠ《〮‰਍㈱㔹㔮‱㈱㐹㠮′㈱㈹㈮‴㈱㜸㐮‰㈱㤷㌮‶㈱㜶㠮‸㈱㈵㌮′਍㈱㌳㈮‱㈱〱ㄮ‰ㄱ㌸ㄮ‷ㄱ㈵〮‵ㄱ㜱㔮′〱㤷㈮‴〱㠳㈮‱਍㤹⸳㌸㤠㜴㐮‰㤸⸹㤰㠠㠴㜮″㤷⸶㜶㜠㌴㌮‸㠶⸸㘵㘠㌳㔮‰਍㜵⸹㐰㔠㔲㠮‹㜴⸴ㄲ㐠㐲〮‹㜳⸵㠶㌠㤲ㄮ‴㠲⸴㜷㈠㌴ㄮ‱਍〲⸴㐵ㄠ㠶㔮′㌱⸵㘴ㄠ㔰㤮‱〸㌮″㠵㠮‹ㄴ㘮‶㤲㈮‷㠱㌮‴਍⸵㠸〠㤮‰⸱㤳ㄠ㘮‷⸱㐸ㄠ㤮‵⸲㌲㈠㔮‱⸲㈸㌠ㄮ‰⸳㔴ഠ㌊㔮‵⸳㈷㌠㤮‷⸴ㄲ㐠㈮‵⸴㔴㐠㘮‶⸴㐸㔠〮‱⸵㤱㔠㐮‶਍⸵㜶㘠〮′⸶㘱㘠㐮‴⸶㈷㜠〮‷⸷㜲㜠㔮′⸷ㄴ㜠㈮‴⸷〱ഠ㘊㤮‶਍,0.9,D71CL+D71/6DL,Luceplan S.r.l.,Sound absorbing panel,332.792986005153,4182.000000000000,1,0,,1,1,Dimmable,"54W center LED module, 3000K, dimmable 0-10V + LED low power strip perimeter for accent (4182 lm delivered)",2,,3000.000000000000,,35.821538886688,2.362204724409,50 - 60 Hz,79.130000000000,0,"Light as a suspended petal, white as the subdued lighting and with a softness that enhances it. A suspension lamp with an organic form which conceals the magic of silence within: the body consists of a sound-absorbent panel upholstered in white fabric.",48.000000000000,47.244094488189,16777215,29.527559055118,29.527559055118,>80,1,1,https://img.edilportale.com/bim/LUCEPLAN-BIM-USER-MANUAL-LUCEPLAN-bim.pdf,https://bim.archiproducts.com/en/badge/bim-archiproducts-featured_658700/about,https://bim.archiproducts.com/,120.000000000000,0.000000000000,https://www.luceplanusa.com/assets/D710IB104_PETALE_UL.pdf,1D71/0AC0002,D71/0AC,A
